("FILE_TYPE"	"PMAP File"
    ("devices"
        ("LEDR")
        ("L"
            ("info"
                ("spice_dsg"	"L")
                ("port_order"
                    ("1")
                    ("2")
                )
            )
            ("model_params"
                ("level_0"
                    ("VALUE"
                        ("value"	"0")
                    )
                )
            )
            ("smoke"
                ("pre_smoke"
                    ("TERM_IA"	"-1")
                    ("NODE_VA"	"1")
                    ("NODE_VB"	"2")
                    ("DERATE_TYPE"	"IND")
                )
                ("max_ops"
                    ("LI"	"CURRENT")
                    ("LV"	"DIELECTRIC")
                )
                ("smoke_tests"
                    ("LI"
                        ("test"	"abs_current_test")
                        ("term"	"TERM_IA")
                    )
                    ("LV"
                        ("test"	"abs_voltage_test")
                        ("nodes"
                            ("NODE_VA")
                            ("NODE_VB")
                        )
                    )
                )
                ("device_max_ops")
            )
        )
        ("C"
            ("info"
                ("spice_dsg"	"C")
                ("port_order"
                    ("1")
                    ("2")
                )
            )
            ("model_params"
                ("level_0"
                    ("IC"
                        ("value"	"0")
                    )
                    ("TC"
                        ("value"	"0")
                    )
                    ("VALUE"
                        ("value"	"0")
                    )
                )
            )
            ("smoke"
                ("pre_smoke"
                    ("NODE_VA"	"1")
                    ("NODE_VB"	"2")
                    ("TERM_A"	"-1")
                    ("DERATE_TYPE"	"CAP")
                )
                ("max_ops"
                    ("CV"	"VOLTAGE")
                    ("CI"	"CURRENT")
                    ("SLP"	"SLOPE")
                    ("TBRK"	"KNEE")
                    ("TMAX"	"MAX_TEMP")
                )
                ("smoke_tests"
                    ("CV"
                        ("test"	"abs_voltage_test")
                        ("nodes"
                            ("NODE_VA")
                            ("NODE_VB")
                        )
                    )
                    ("CI"
                        ("test"	"abs_current_test")
                        ("term"	"TERM_A")
                    )
                )
                ("device_max_ops")
            )
        )
        ("R"
            ("info"
                ("spice_dsg"	"R")
                ("port_order"
                    ("1")
                    ("2")
                )
            )
            ("model_params"
                ("level_0"
                    ("TC1"
                        ("value"	"0")
                    )
                    ("TC2"
                        ("value"	"0")
                    )
                    ("VALUE"
                        ("value"	"0")
                    )
                )
            )
            ("smoke"
                ("pre_smoke"
                    ("NODE_VA"	"1")
                    ("NODE_VB"	"2")
                    ("DERATE_TYPE"	"RES")
                )
                ("max_ops"
                    ("RV"	"VOLTAGE")
                    ("PDM"	"POWER")
                    ("SLP"	"SLOPE")
                    ("RBA"	"1/SLP")
                    ("TMAX"	"MAX_TEMP")
                    ("TB"	"TMAX")
                    ("RTKNEE"	"TKNEE")
                    ("RTRISE"	"TRISE")
                )
                ("smoke_tests"
                    ("PDM"
                        ("test"	"power_test")
                    )
                    ("RV"
                        ("test"	"abs_voltage_test")
                        ("nodes"
                            ("NODE_VA")
                            ("NODE_VB")
                        )
                    )
                    ("TB"
                        ("test"	"temp_null_test")
                    )
                )
                ("device_max_ops")
            )
        )
        ("B240A")
        ("VPULSE")
        ("AL8841Q")
    )
    ("instances"
        ("U6"
            ("device_name"	"LEDR")
            ("pspice_path"	"X_U6")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("AREA"
                    ("value"	"")
                    ("pspice_param"	"AREA")
                )
            )
        )
        ("U8"
            ("device_name"	"LEDR")
            ("pspice_path"	"X_U8")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("AREA"
                    ("value"	"")
                    ("pspice_param"	"AREA")
                )
            )
        )
        ("U7"
            ("device_name"	"LEDR")
            ("pspice_path"	"X_U7")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("AREA"
                    ("value"	"")
                    ("pspice_param"	"AREA")
                )
            )
        )
        ("L1"
            ("device_name"	"L")
            ("pspice_path"	"L_L1")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"68u")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
                ("IC"
                    ("value"	"0")
                    ("pspice_param"	"IC")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("CURRENT"
                    ("value"	"LMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("DIELECTRIC"
                    ("value"	"DSMAX")
                    ("pspice_param"	"DIELECTRIC")
                )
                ("IL1"
                    ("value"	"0")
                    ("pspice_param"	"IL1")
                )
                ("IL2"
                    ("value"	"0")
                    ("pspice_param"	"IL2")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
            ("smoke_vars"
                ("CURRENT"	"5.0")
                ("DIELECTRIC"	"300.0")
            )
        )
        ("C6"
            ("device_name"	"C")
            ("pspice_path"	"C_C6")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1n")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("VC1"
                    ("value"	"0")
                    ("pspice_param"	"VC1")
                )
                ("VC2"
                    ("value"	"0")
                    ("pspice_param"	"VC2")
                )
            )
            ("smoke_vars"
                ("VOLTAGE"	"50.0")
                ("CURRENT"	"1.0")
                ("SLOPE"	"0.005")
                ("KNEE"	"125.0")
                ("MAX_TEMP"	"125.0")
            )
        )
        ("C4"
            ("device_name"	"C")
            ("pspice_path"	"C_C4")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"100n")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
                ("IC"
                    ("value"	"0")
                    ("pspice_param"	"IC")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("VC1"
                    ("value"	"0")
                    ("pspice_param"	"VC1")
                )
                ("VC2"
                    ("value"	"0")
                    ("pspice_param"	"VC2")
                )
            )
            ("smoke_vars"
                ("VOLTAGE"	"50.0")
                ("CURRENT"	"1.0")
                ("SLOPE"	"0.005")
                ("KNEE"	"125.0")
                ("MAX_TEMP"	"125.0")
            )
        )
        ("C5"
            ("device_name"	"C")
            ("pspice_path"	"C_C5")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"4.7u")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
                ("IC"
                    ("value"	"0")
                    ("pspice_param"	"IC")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("VC1"
                    ("value"	"0")
                    ("pspice_param"	"VC1")
                )
                ("VC2"
                    ("value"	"0")
                    ("pspice_param"	"VC2")
                )
            )
            ("smoke_vars"
                ("VOLTAGE"	"50.0")
                ("CURRENT"	"1.0")
                ("SLOPE"	"0.005")
                ("KNEE"	"125.0")
                ("MAX_TEMP"	"125.0")
            )
        )
        ("R1"
            ("device_name"	"R")
            ("pspice_path"	"R_R1")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"0.1")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
            ("smoke_vars"
                ("POWER"	"0.25")
                ("SLOPE"	"0.005")
                ("MAX_TEMP"	"200.0")
            )
        )
        ("D1"
            ("device_name"	"B240A")
            ("pspice_path"	"X_D1")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("AREA"
                    ("value"	"")
                    ("pspice_param"	"AREA")
                )
            )
        )
        ("VCTRL"
            ("device_name"	"VPULSE")
            ("pspice_path"	"V_VCTRL")
            ("level"	"0")
            ("model_params"
                ("V2"
                    ("value"	"3.3")
                    ("pspice_param"	"V2")
                )
                ("V1"
                    ("value"	"0")
                    ("pspice_param"	"V1")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("PER"
                    ("value"	"")
                    ("pspice_param"	"PER")
                )
                ("PW"
                    ("value"	"")
                    ("pspice_param"	"PW")
                )
                ("TF"
                    ("value"	"")
                    ("pspice_param"	"TF")
                )
                ("TR"
                    ("value"	"")
                    ("pspice_param"	"TR")
                )
                ("TD"
                    ("value"	"")
                    ("pspice_param"	"TD")
                )
                ("AC"
                    ("value"	"")
                    ("pspice_param"	"AC")
                )
                ("DC"
                    ("value"	"")
                    ("pspice_param"	"DC")
                )
            )
        )
        ("VIN"
            ("device_name"	"VPULSE")
            ("pspice_path"	"V_VIN")
            ("level"	"0")
            ("model_params"
                ("TR"
                    ("value"	"3m")
                    ("pspice_param"	"TR")
                )
                ("V2"
                    ("value"	"25")
                    ("pspice_param"	"V2")
                )
                ("V1"
                    ("value"	"0")
                    ("pspice_param"	"V1")
                )
                ("TD"
                    ("value"	"100n")
                    ("pspice_param"	"TD")
                )
                ("PER"
                    ("value"	"")
                    ("pspice_param"	"PER")
                )
                ("PW"
                    ("value"	"")
                    ("pspice_param"	"PW")
                )
                ("TF"
                    ("value"	"")
                    ("pspice_param"	"TF")
                )
                ("AC"
                    ("value"	"")
                    ("pspice_param"	"AC")
                )
                ("DC"
                    ("value"	"")
                    ("pspice_param"	"DC")
                )
            )
        )
        ("U9"
            ("device_name"	"AL8841Q")
            ("pspice_path"	"X_U9")
            ("level"	"0")
            ("model_params"
                ("TEMP_CHANGE_RATE"
                    ("value"	"500U")
                    ("pspice_param"	"TEMP_CHANGE_RATE")
                )
                ("TAMB"
                    ("value"	"27")
                    ("pspice_param"	"TAMB")
                )
                ("RTJA"
                    ("value"	"56")
                    ("pspice_param"	"RTJA")
                )
            )
        )
    )
)
