
**** 09/04/24 15:07:52 ***** PSpice 22.1.0 (28 June 2024) ***** ID# 0 ********

 ** Profile: "STARTUP-TRANS"  [ D:\Diodes\login\LED\AL8841\Simulation\Pspice\AL8841Q-Pspice model\Encrypted\AL8841Q_MSOP8\al8841q-psp


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "TRANS.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Profile Libraries :
* Local Libraries :
.LIB "D:/Diodes/login/LED/AL8841/Simulation/Pspice/AL8841Q-Pspice model/Encrypted/al8841_msop8/al8841q.lib" 
* From [PSPICE NETLIST] section of C:\Users\rock_chiu024\AppData\Roaming\SPB_Data\cdssetup\OrCAD_PSpice\22.1.0\PSpice.ini file:

ERROR(ORPSIM-16276): Simulation cannot be completed because library D:/Diodes/login/LED/AL8841/Simulation/Pspice/AL8841Q-Pspice model/Encrypted/al8841_msop8/al8841q.lib 
is not available.
.lib "nom.lib" 

*Analysis directives: 
.TRAN  0 3.5m 0 20n 
.OPTIONS ADVCONV
.OPTIONS ABSTOL= 1.0n
.OPTIONS ITL4= 100
.PROBE64 V(alias(*)) I(alias(*)) 
.INC "..\STARTUP.net" 



**** INCLUDING STARTUP.net ****
* source AL8841Q
X_U6         SET N90786 LEDR
X_U8         N90814 N90842 LEDR
X_U7         N90786 N90814 LEDR
L_L1         N90842 SW  68u IC=0 
C_C6         N90842 SET  1n  TC=0,0 
C_C4         0 VIN  100n IC=0 TC=0,0 
C_C5         0 VIN  4.7u IC=0 TC=0,0 
R_R1         SET VIN  0.1 TC=0,0 
X_D1         SW VIN B240A
V_VCTRL         CTRL 0  
+PULSE 0 3.3 0 
V_VIN         VIN 0  
+PULSE 0 25 100n 3m 
X_U9         0 0 SET NC CTRL VIN SW AL8841Q PARAMS:  TEMP_CHANGE_RATE=500U
+  TAMB=27 RTJA=56

**** RESUMING TRANS.cir ****
.END
